<ASSEMBLER_INFO>
 <VERSION>2.1.42</VERSION>
 <DEVICE>ATmega8515</DEVICE>
 <WORKING_DIR>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515</WORKING_DIR>
 <INCLUDE_PATH>
  <DIR>C:\Program Files (x86)\Atmel\AVR Tools\AvrAssembler2\Appnotes</DIR>
 </INCLUDE_PATH>
 <SOURCE_FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</SOURCE_FILE>
 <INCLUDED_FILES>
  <FILE>C:\Program Files (x86)\Atmel\AVR Tools\AvrAssembler2\Appnotes\m8515def.inc</FILE>
 </INCLUDED_FILES>
 <OBJECT_FILES>
  <FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.obj</FILE>
 </OBJECT_FILES>
 <HEX_FILES>
  <FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.hex</FILE>
 </HEX_FILES>
 <OUTPUT_FILES>
  <FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.map</FILE>
 </OUTPUT_FILES>
 <LABELS>
  <RESET><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>417</LINE></RESET>
  <i2c_hp_delay><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>99</LINE></i2c_hp_delay>
  <i2c_hp_delay_loop><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>101</LINE></i2c_hp_delay_loop>
  <i2c_qp_delay><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>106</LINE></i2c_qp_delay>
  <i2c_qp_delay_loop><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>108</LINE></i2c_qp_delay_loop>
  <i2c_rep_start><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>133</LINE></i2c_rep_start>
  <i2c_start><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>160</LINE></i2c_start>
  <i2c_write><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>186</LINE></i2c_write>
  <i2c_write_first><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>192</LINE></i2c_write_first>
  <i2c_write_bit><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>190</LINE></i2c_write_bit>
  <i2c_get_ack><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>227</LINE></i2c_get_ack>
  <i2c_write_low><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>200</LINE></i2c_write_low>
  <i2c_write_high><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>203</LINE></i2c_write_high>
  <i2c_get_ack_wait><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>233</LINE></i2c_get_ack_wait>
  <i2c_do_transfer><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>266</LINE></i2c_do_transfer>
  <i2c_read><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>293</LINE></i2c_read>
  <i2c_read_bit><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>297</LINE></i2c_read_bit>
  <i2c_put_ack><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>328</LINE></i2c_put_ack>
  <i2c_put_ack_low><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>335</LINE></i2c_put_ack_low>
  <i2c_put_ack_high><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>337</LINE></i2c_put_ack_high>
  <i2c_put_ack_wait><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>341</LINE></i2c_put_ack_wait>
  <i2c_stop><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>364</LINE></i2c_stop>
  <i2c_init><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>399</LINE></i2c_init>
  <main><FILE>E:\WORK\electronica\EC1204B Banggood watch\Software ATMega8515\avr300.asm</FILE><LINE>418</LINE></main>
 </LABELS>
</ASSEMBLER_INFO>
